1.1                          A bill for an act
  1.2             relating to corrections; modifying multiple occupancy 
  1.3             requirements applicable to state prisons; amending 
  1.4             Minnesota Statutes 1996, section 243.53. 
  1.5   BE IT ENACTED BY THE LEGISLATURE OF THE STATE OF MINNESOTA: 
  1.6      Section 1.  Minnesota Statutes 1996, section 243.53, is 
  1.7   amended to read: 
  1.8      243.53 [SEPARATE CELLS; MULTIPLE OCCUPANCY STANDARDS.] 
  1.9      Subdivision 1.  [SEPARATE CELLS.] When there are cells 
  1.10  sufficient, each convict inmate shall be confined in a separate 
  1.11  cell.  Each inmate shall be confined in a separate cell 
  1.12  in close, maximum, and high security facilities, including St. 
  1.13  Cloud, Stillwater, and Oak Park Heights institutions classified 
  1.14  by the commissioner as custody level five and six institutions, 
  1.15  but not including geriatric or honor dormitory-type facilities. 
  1.16     Subd. 2.  [MULTIPLE OCCUPANCY STANDARDS.] A medium security 
  1.17  correctional facility that is built or remodeled after July 1, 
  1.18  1992, for the purpose of increasing inmate capacity must be 
  1.19  designed and built to comply with multiple occupancy standards 
  1.20  for not more than one-half of the facility's 
  1.21  capacity Correctional institutions classified by the 
  1.22  commissioner as custody level one, two, three, or four 
  1.23  institutions must permit double celling to the greatest extent 
  1.24  possible, comply with multiple occupancy standards, and must 
  1.25  include a maximum capacity figure.  A minimum security 
  2.1   correctional facility that is built or remodeled after July 1, 
  2.2   1992, must be designed and built to comply with minimum security 
  2.3   multiple occupancy standards. 
  2.4      Sec. 2.  [EFFECTIVE DATE.] 
  2.5      Section 1 is effective the day following final enactment.