1.1 	A bill for an act
1.2 	relating to high pressure piping; classifying data relating to bioprocess piping 
1.3 	and equipment as nonpublic; including bioprocess piping in the definition of 
1.4 	high pressure piping;amending Minnesota Statutes 2004, sections 16B.61, 
1.5 	subdivisions 2, 3; 326.461, subdivision 2; proposing coding for new law in 
1.6 	Minnesota Statutes, chapter 13.
1.7 	BE IT ENACTED BY THE LEGISLATURE OF THE STATE OF MINNESOTA:

1.8 	Section 1. [13.7911] BIOPROCESS PIPING AND EQUIPMENT DATA.
1.9 	All data regarding the material production processes, including the bioprocess 
1.10 	system's structural design and layout, are classified as nonpublic data. Bioprocess piping 
1.11 	and equipment are limited to those used in the creation of a product utilizing living 
1.12 	organisms for medical, research, or pharmaceutical purposes and meeting the most current 
1.13 	requirements in the bioprocessing equipment standard adopted by the American Society 
1.14 	of Mechanical Engineers.

1.15 	Sec. 2. Minnesota Statutes 2004, section 16B.61, subdivision 2, is amended to read:
1.16 		Subd. 2.Enforcement by certain bodies. Under the direction and supervision of 
1.17 	the commissioner, the provisions of the code relating to electrical installations shall be 
1.18 	enforced by the State Board of Electricity, pursuant to the Minnesota Electrical Act, the 
1.19 	provisions relating to plumbing shall be enforced by the commissioner of health, the 
1.20 	provisions relating to high pressure steam piping and appurtenances, ammonia piping, and 
1.21 	bioprocess piping shall be enforced by the Department of Labor and Industry. Fees for 
1.22 	inspections conducted by the State Board of Electricity shall be paid in accordance with 
1.23 	the rules of the State Board of Electricity. Under direction of the commissioner of public 
1.24 	safety, the state fire marshal shall enforce the Minnesota Uniform Fire Code as provided 
2.1 	in chapter 299F. The commissioner, in consultation with the commissioner of labor and 
2.2 	industry, shall adopt amendments to the mechanical code portion of the State Building 
2.3 	Code to implement standards for process piping.

2.4 	Sec. 3. Minnesota Statutes 2004, section 16B.61, subdivision 3, is amended to read:
2.5 		Subd. 3.Special requirements. (a) Space for commuter vans. The code must 
2.6 	require that any parking ramp or other parking facility constructed in accordance with the 
2.7 	code include an appropriate number of spaces suitable for the parking of motor vehicles 
2.8 	having a capacity of seven to 16 persons and which are principally used to provide 
2.9 	prearranged commuter transportation of employees to or from their place of employment 
2.10 	or to or from a transit stop authorized by a local transit authority. 
2.11 	(b)  Smoke detection devices. The code must require that all dwellings, lodging 
2.12 	houses, apartment houses, and hotels as defined in section  299F.362 comply with the 
2.13 	provisions of section  299F.362. 
2.14 	(c)  Doors in nursing homes and hospitals. The State Building Code may not 
2.15 	require that each door entering a sleeping or patient's room from a corridor in a nursing 
2.16 	home or hospital with an approved complete standard automatic fire extinguishing system 
2.17 	be constructed or maintained as self-closing or automatically closing. 
2.18 	(d)  Child care facilities in churches; ground level exit. A licensed day care center 
2.19 	serving fewer than 30 preschool age persons and which is located in a belowground space 
2.20 	in a church building is exempt from the State Building Code requirement for a ground 
2.21 	level exit when the center has more than two stairways to the ground level and its exit. 
2.22 	(e)  Child care facilities in churches; vertical access. Until August 1, 1996, an 
2.23 	organization providing child care in an existing church building which is exempt from 
2.24 	taxation under section  272.02, subdivision 6, shall have five years from the date of initial 
2.25 	licensure under chapter 245A to provide interior vertical access, such as an elevator, to 
2.26 	persons with disabilities as required by the State Building Code. To obtain the extension, 
2.27 	the organization providing child care must secure a $2,500 performance bond with the 
2.28 	commissioner of human services to ensure that interior vertical access is achieved by the 
2.29 	agreed upon date. 
2.30 	(f)  Family and group family day care. Until the legislature enacts legislation 
2.31 	specifying appropriate standards, the definition of Group R-3 occupancies in the State 
2.32 	Building Code applies to family and group family day care homes licensed by the 
2.33 	Department of Human Services under Minnesota Rules, chapter 9502. 
3.1 	(g)  Enclosed stairways. No provision of the code or any appendix chapter of the 
3.2 	code may require stairways of existing multiple dwelling buildings of two stories or 
3.3 	less to be enclosed. 
3.4 	(h)  Double cylinder dead bolt locks. No provision of the code or appendix chapter 
3.5 	of the code may prohibit double cylinder dead bolt locks in existing single-family homes, 
3.6 	townhouses, and first floor duplexes used exclusively as a residential dwelling. Any 
3.7 	recommendation or promotion of double cylinder dead bolt locks must include a warning 
3.8 	about their potential fire danger and procedures to minimize the danger. 
3.9 	(i)  Relocated residential buildings. A residential building relocated within or 
3.10 	into a political subdivision of the state need not comply with the State Energy Code or 
3.11 	section  326.371 provided that, where available, an energy audit is conducted on the 
3.12 	relocated building. 
3.13 	(j)  Automatic garage door opening systems. The code must require all residential 
3.14 	buildings as defined in section  325F.82 to comply with the provisions of sections  325F.82
3.15 	and  325F.83. 
3.16 	(k)  Exit sign illumination. For a new building on which construction is begun 
3.17 	on or after October 1, 1993, or an existing building on which remodeling affecting 50 
3.18 	percent or more of the enclosed space is begun on or after October 1, 1993, the code must 
3.19 	prohibit the use of internally illuminated exit signs whose electrical consumption during 
3.20 	nonemergency operation exceeds 20 watts of resistive power. All other requirements in 
3.21 	the code for exit signs must be complied with. 
3.22 	(l)  Exterior wood decks, patios, and balconies. The code must permit the decking 
3.23 	surface and upper portions of exterior wood decks, patios, and balconies to be constructed 
3.24 	of (1) heartwood from species of wood having natural resistance to decay or termites, 
3.25 	including redwood and cedars, (2) grades of lumber which contain sapwood from species 
3.26 	of wood having natural resistance to decay or termites, including redwood and cedars, or 
3.27 	(3) treated wood. The species and grades of wood products used to construct the decking 
3.28 	surface and upper portions of exterior decks, patios, and balconies must be made available 
3.29 	to the building official on request before final construction approval. 
3.30 	(m) Bioprocess piping and equipment. All data regarding the material production 
3.31 	processes, including the bioprocess system's structural design and layout, are trade secret 
3.32 	information under section 13.37 and nonpublic data under section 13.7911. Bioprocess 
3.33 	piping and equipment are limited to those used in the creation of a product utilizing 
3.34 	living organisms for medical, research, or pharmaceutical purposes and meeting the most 
3.35 	current requirements set forth in the bioprocessing equipment standards adopted by the 
3.36 	American Society of Mechanical Engineers. No permit fee for bioprocess piping may be 
4.1 	imposed by municipalities under the State Building Code, except as required under section 
4.2 	326.47, subdivision 1. Permits for bioprocess piping shall be according to section 326.47 
4.3 	administered by the Department of Labor and Industry.

4.4 	Sec. 4. Minnesota Statutes 2004, section 326.461, subdivision 2, is amended to read:
4.5 		Subd. 2.High pressure piping. "High pressure piping" means all high pressure 
4.6 	piping used in the installation of hot water or steam heating boilers, any systems of piping 
4.7 	hot water or other medium used for heating that exceed 30 p.s.i. gauge and 250 degrees 
4.8 	Fahrenheit, or any system of high pressure steam or, ammonia piping, or bioprocess 
4.9 	piping, but shall not include any high pressure piping under the direct jurisdiction of 
4.10 	the United States.